/////////////////////////////////////////////////////////////////////////////
//////                                                                 //////
//////   Billion Vista ISDN Driver Package v1_0   Feb 14th 2007        //////
//////                                                                 //////
/////////////////////////////////////////////////////////////////////////////



!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

This software is supplied FOR TESTING + EVALUATION PURPUSES ONLY !

This software must be treated as CONFIDENTIAL and must not be given to 
any third party outside of Billion and Stollmann nor to any end user.

This software is supplied "as is"; anybody using this software does so 
on their own risk !

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

Please read this document before using the software.

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!




A. PACKAGE CONTENTS


The Disk-Folder contents represents the end user installation CD contents.
At the same time, Setup.exe represents the "Software First" executable to be 
distributed via the internet and via Windows Update.



B. USAGE


1. Test System Setup
Use a PC with 32BIT or 64BIT Windows XP SP2 or Windows Vista installed.
This driver package has been signed with the Stollmann certificate. For 
a final product if the driver is WHQL-signed by Microsoft, the Stollmann
certificate is not needed anymore.

By using 64BIT Windows systems an additional test setup is required:
- Open a command line Start->Run->Cmd.exe
- Use the command "BCEDIT -set testsigning on" 
- Reboot the PC
- The system restarts in test mode with a small "test mode" brand on the top 
  on each corner of the display and the system version/build on the top line 
  of the display in the center.


2. Installation
- Execute Setup.exe.
- Click "Finish".
- Connect a Billion ISDN device (USB or PCI).


3. Evaluation
- Perform a self test via the taskbar icon's "Self Test" menu.
- Set up a RAS connection using the ISDN WAN Device.



C. KNOWN RESTRICTIONS

- ISDN FAX Modem not included in this package
