=====================================================

					Au9520 Linux RPM Package Release Note				      
					
=====================================================					

v1.0.0  2006/09/04

The ccid driver is based on pcsclib, and pcsc-lite.
If the version of the libusb is under ver 0.1.7 then libusb need to update

First install libusb
#rpm -ivh libusb-0.1.12-1.i386.rpm

Second install pcsc-lite
#rpm -ivh pcsc-lite-1.3.2-1.i386.rpm

Finally install ccid driver
#rpm -ivh ccid-1.1.0-1.i386.rpm

Activate the pcscd daemon
 #/usr/local/sbin/pcscd

Test tool:
The formaticc can send batch APDUs to smartcard.
Execute the followint instruction



You can use "Formaticc" to send batch APDUs
Execute  /pcsc-lite-1.3.2/src/utils/formaticc

[Example]
[root@localhost utils]# ./formaticc

Winscard PC/SC Lite Test Program

Please enter the desired host (localhost for this machine) [localhost]:
Please input the desired transmit protocol (0/1) [0]:
Please input the desired input apdu file: sample.in
[root@localhost utils]# ./formaticc

Winscard PC/SC Lite Test Program

Please enter the desired host (localhost for this machine) [localhost]:
Please input the desired transmit protocol (0/1) [0]:
Please input the desired input apdu file: sample.in
Please input the desired output apdu file: 123.out
Reader 01: Alcor Micro AU9520 00 00
Enter the desired reader number: 01

Please insert a smart card
Processing Command 001 of length 005: 05 C0 84 00 00 08
Processing Command 002 of length 005: 05 C0 84 00 00 08
Processing Command 003 of length 007: 07 C0 A4 00 00 02 3F 00
Processing Command 004 of length 007: 07 C0 A4 00 00 02 3F 00

[root@localhost utils]# vi 123.out

Content of file 123.out 
02 6E 00
02 6E 00
02 6E 00
02 6E 00