=====================================================

					Au9520 Linux RPM Package Release Note				      
					
=====================================================					

v1.0.0  2006/09/04

The ccid driver is based on pcsclib, and pcsc-lite.
If the version of the libusb is under ver 0.1.7 then libusb need to update

First install libusb
#rpm -ivh libusb-0.1.12-1.i386.rpm

Second install pcsc-lite
#rpm -ivh pcsc-lite-1.3.2-1.i386.rpm

Finally install ccid driver
#rpm -ivh ccid-1.1.0-1.i386.rpm

Activate the pcscd daemon
 #/usr/local/sbin/pcscd

Test tool:
The formaticc can send batch APDUs to smartcard.
Execute the followint instruction

The input file format as follows:

Length   APDUs
05            00 84 00 00 08

05 is the APDU's length ,and 00 84 00 00 08 is the APDU command.

You can use "Formaticc" to send batch APDUs
Execute  /pcsc-lite-1.3.2/src/utils/formaticc

[Example]
[root@localhost utils]# ./formaticc

Winscard PC/SC Lite Test Program

Please enter the desired host (localhost for this machine) [localhost]:
Please input the desired transmit protocol (0/1) [0]:
Please input the desired input apdu file: sample.in
[root@localhost utils]# ./formaticc

Winscard PC/SC Lite Test Program

Please enter the desired host (localhost for this machine) [localhost]:
Please input the desired transmit protocol (0/1) [0]:
Please input the desired input apdu file: sample.in
Please input the desired output apdu file: 123.out
Reader 01: Alcor Micro AU9520 00 00
Enter the desired reader number: 01

Please insert a smart card
Processing Command 001 of length 005: 05 C0 84 00 00 08
Processing Command 002 of length 005: 05 C0 84 00 00 08
Processing Command 003 of length 007: 07 C0 A4 00 00 02 3F 00
Processing Command 004 of length 007: 07 C0 A4 00 00 02 3F 00

[root@localhost utils]# vi 123.out

Content of file 123.out 
02 6E 00
02 6E 00
02 6E 00
02 6E 00